Computer Science and Artificial Intelligence

COC 257

B822620

**Autonomous Car Simulation**

*by*

*Kieran M. Apps*

*Supervisor: Dr. Shaheen Fatima*

*Department of Computer Science*

*Loughborough University*

June 2022

Autonomous Car Simulation

Kieran Apps (B822620)

Loughborough University



Table of Contents

1. Introduction and Description
   * + 1. Brief Description
       2. Aims and Objectives
       3. Short Summary of the Project
2. Literature Review
   1. Machine Learning Methodologies; Supervised, Unsupervised, Reinforcement and Evolutionary
   2. Neural Networks and Deep Learning
   3. Genetic Algorithms (2.3.1) and NEAT (2.3.2)
   4. Methods for Automated Vehicles
3. Methodology Used
4. Implementation
5. Results
6. Conclusion and Further Work
7. References

Section 1: Introduction and Description

1.1 Brief Description

Choosing this project was relatively easy for me, cars are a big passion of mine, and the area of self-driving and autonomous cars has exploded in popularity in the recent years, with the likes of Tesla and their own Autopilot system in their vehicles.

Creating this project will give me great knowledge of this new emergent field of A.I. and allow me the learn and practically try out some of the key techniques that are used to create autonomous driving systems. The project itself will be a simulation of an autonomous car using Unity to host the simulated environment, track and car itself, then, Python will be used to program the Artificial Intelligence used to control the cars actions thanks to its useful libraries and lots of support around the language for A.I..

Using this combination plays both to my strengths of my knowledge of Python already and allows me to explore a new area of Python, that being the A.I and Machine Learning side of the language, as well as explore a new language C# with Unity. Thus, developing my skills of developing A.I and learning new language quickly and efficiently such that I can implement the simulation needed.

I believe this project will also allow me to explore some Machine Learning and A.I. techniques that truly interest me, allowing me to develop a deep understanding of such techniques so that I will be able to apply them to many other fields. On top of exploring the new aspects of A.I. that I have not previously been exposed to, I will also be able to collect some knowledge from previous University modules into this one task proving that I can apply what was previously taught to a new situation.

For the track that the car will have to navigate, I will be taking a real racetrack found in northern England called Cadwell Park, this way, I can ensure a wide variety of corner types, angle as well as some lengthy straights for the car to adapt to. Not only does it ensure a wide range of corners for the car to learn, but it will allow for a direct comparison to real cars on the same track such that we can see how similarly this A.I. performed to real experienced drivers on the same track. The car will likely not behave in precisely the same way; however, this comparison could give some extremely useful insight into the next steps of the car, and the current successes that the car made within this project.

1.2 Aims and Objectives

My main task for this project is to create a successful autonomous vehicle that can navigate a predefined track successfully avoiding any collisions with the track itself (i.e., without hitting any walls). Building on from this base task, I want to try and create a car that is able to navigate the course at speed, meaning that the vehicle is able to learn to accelerate and decelerate (or brake) for corners and straights, rather than the car just maintaining one constant slow speed to travel around the track.

There have been previous papers and projects exploring the simulation of an autonomous vehicle, however, most of these projects aim for the base case that I want to achieve, this being a car that can navigate around a predefined track safely without colliding with any of the environment. Alternatively, these projects used a slightly different case which is navigating around in a traffic light environment meaning following road laws, signs and potentially even avoiding collisions with other motorists.

My project differs in the aspect that I want to achieve a more advanced car that as mentioned, is able to understand a path and use this knowledge to accelerate and brake accordingly to provide a faster lap, whilst also remaining safe and avoiding the environment.

I also plan to have the car ‘see’ in a similar way to which real autonomous vehicles ‘see’ using Lidar by implementing a similar method into the simulation to gather data about the environment that the car will use to navigate.

In a simplified bullet point list, the progress and objectives will be as follows, from the most basic and beginning of the project, to implementing the A.I. into the car:

* Create 3D model of Cadwell Park
* Create Unity project, load in the track and create a car model
* Create the car controller
* Create all of the event handling within Unity (for collisions, resetting the car and maintain knowledge of the current world state)
* Start the Python side of the project
* Add in a WebSocket to both Unity and Python
* Set up the Neural Network generation and forward pass
* Implement the Genetic Algorithm (this choice will be explained further in this report)
* Train the cars using a multitude of different network topologies
* Analyse the performance of these different topologies

1.3 Short Summary of the Project

All in all, I will be developing an autonomous car simulation using the latest methods in Artificial Intelligence such as Deep Neural Networks (Deep Learning) and Genetic Algorithms to help evolve the car into a safe, effective and fast autonomous vehicle which then will be comparable to a nearly identical real-world scenario to find the strengths, weaknesses and improvements needed for this A.I. system.

Section 2: Literature Review

As part of this project, a considerable amount of research into relevant and potential methods on how to create, control and train the A.I. of the car was undertaken. Outlined in this section is a report on all of my findings and how they can be applied to this area of Artificial Intelligence.

2.1 Machine Learning Methodologies; Supervised, Unsupervised, Reinforcement and Evolutionary:

In machine learning, there are numerous ways for a computer to ‘learn’, these main methods being Supervised and Unsupervised learning. Each of these methods has its benefits and drawbacks as well as being more applicable to certain applications that to others.

Supervised Learning:

Supervised learning is the most common type of learning in the Machine Learning space currently and as a result has many algorithms associated with it. This method relies on having knowledge of a data set provided [1] and then uses this knowledge, after making its own predictions, to adjust the parameters within the network using a concept known as back propagation [2] so that the next predictions it makes will be more in line with what is actually labeled/categorized within the data set.

We can use this method to help classify areas within an image that the car/vehicle is using to see to help defined certain objects within the image. For example, the roadway can be given as training data [3] and used to teach the machine, thus the car, where it is allowed to navigate to, as well as where within this navigable space is free from obstructions. Not only is this method useful for classification of roadways, but also pedestrian detection can be performed using this method [4].

Convolution Neural Networks (CNNs) are most typically used to process and perform the object detection and classification of these types of images. This type of network is extremely similar to the usual Neural Network architecture in that there are many layers of neurons connected by weighted edges [5] however, the convolution layers usually behave differently in how they achieve their own output values and is also mainly used to process images. These layers take the image and pass a filter over each of the pixel values in the form of a matrix to produce the output of that convolution and convolution layer. A typical filter size is 3x3, hence, this will also shrink the image size on output.

Therefore, supervised learning with the aid of a CNN is a potential combination of techniques to allow a car to know where to drive and recognize objects of importance within its field of view, such as sign posts, pedestrians and other cars allowing it to then make decisions on where to navigate to.

Overall, this method of taking video from a vehicle and analysing it to perform a whole manner of operations like segmentation (finding the drivable area, as described) and object detection (such as for pedestrians) [6] is widely used in the pursuit of autonomous vehicles.

Unsupervised Learning:

Usually, unsupervised learning is used in a case where there is an extremely large volume of data provided to a system and is unlabeled or uncategorised.

Within this method there are again lots of different techniques and algorithms that can be applied to better fit the situation that it will be used in with some of the most widely known being Hierarchical Learning and Data Clustering [7].

Data Clustering [8] is perhaps one of the most popular methods of this learning type and is used to find patterns throughout a large set of unlabeled data and then use this to group (cluster) together similar points of data. One method for this type of clustering is k-means clustering. K-means clustering [9] uses a point called a centroid which upon initialization are randomly placed within the data space then used to calculate the Euclidian distance to all other points with these points then assigned to the cluster centroid closest to them. After this, the centroid is recalculated to be the centre of the cluster created and the process repeats. The process repeats k times, hence k-means, since this method can be prone to converging in an undesirable location, or local optima, so running multiple times can help relieve this issue to gain a result that will be successful enough in a practical scenario.

These types of methods however cannot easily be applied to an autonomous driving scenario as this is mostly a data mining technique which under the circumstances of an autonomous vehicle would not aid in creating a safe and efficient self-driving machine.

Reinforcement Learning:

Reinforcement learning at its core is very similar to trial and error [34], where an agent tries many different options available to it and is given a value called a reward (calculated using a reward function) depending on how beneficial this action is to the system.

The value function considers the expected/predicted, accumulative, discounted and future reward of any action from the current state that the agent is in. Using this, one of these actions is taken. Usually, the best, or most rewarding action will be taking, which is known as a greedy option, alternatively, some reinforcement algorithms use a probability to determine whether some other action that may not be optimal is taken. This technique of choosing an action is called ε-greedy [35], where ε is the probability of some other, non-optimal action being taken. Choosing either of these options is given a name: Exploitation (picking the best, greedy option) and Exploration (not picking the greedy, and as the name suggests, exploring the space).

As rewards for given actions is certain states are calculated the agent is knowledgeable enough to choose accurately the best option for its current state.

A simple example of reinforcement learning in practice is a simple robot trying to find the exit of a maze. Any action the robot takes that moves it closer to the exit gives a reward, and an action further away gives none, or a smaller reward. As time progresses and the robot explores, the matrix of reward-actions is filled the best values of reward for each action in a current state. Q-learning [36], and functions within this method are used to calculate the values within this matrix and is based on some knowledge of other rewards in states that can be reached from any other state.

Evolutionary:

Evolutionary learning is a relatively new technique within the Artificial Intelligence space and at its core, takes inspiration from the concept of Darwinian evolution [10] and applies this to the Neural Networks or systems that need to be taught to perform a certain task. Because of this inspiration from nature and the natural path of evolution that life takes, a way to judge and discriminate against different individuals in a population must be conceived so that only the best can move forward to produce the next generation, thus improving the A.I.’s ability to perform the given task.

The function required to determine this performance is called a fitness function and is used to perform the fitness evaluation of each individual which then allows for the reproduction of these best individuals to take place.

Reproduction, as the name suggests, is creating a new set of individuals (reproducing them) to populate the next generation, however this itself does come with some challenges. Firstly, is the method to perform this reproduction, and the second is how to prevent the individuals from becoming too similar too quickly and thus not being able to explore a large enough search space to find acceptable results. To combat these issues, cross-over and mutation [11] can be implemented into an evolutionary algorithm to reproduce the individuals chosen during fitness evaluation.

Cross-over:

Crossover is the act of taking a gene/chromosome from one of the parents in the set that passed the fitness evaluation the best and using this to ‘split’ the two parents into two separate genome sequences. After this point is chosen the two parents swap portions to mix together their chromosomes creating this child individual in the new population.

Another way to perform cross-over is with uniform cross-over which is where single chromosomes of an individual are randomly taken from one of the parents and placed into the child individual at the same point this gene was taken from.

Figure: 1 (Showing uniform crossover)

Text, letter

Description automatically generated

Here (Figure 1, above) you can clearly see that with uniform cross-over for the first gene in the sequence of Child One is taken from Parent One and the second in Child One is from Parent Two.

Mutation:

Mutation is used to at random, change the value in any specified slot in a genome of an induvial during the cross-over phase of reproduction to any other valid value. The rate at which mutations occur can be variable and given by a value such as 0.1 to mean a 10% chance that a mutation will occur for this individual.

For a binary individual, such as Figure 1 and Figure 2, the mutation is as simple as flipping a bit from 1 to 0, or 0 to 1. In more complex examples such as a Neural Network the value can be a replacement of a weight or bias to a new random value within the specified range that these weights and biases can exist in, for example, between 0 & 1 or -1 & 1 are some commonly used values.

Figure: 2 (Showing mutation)

Graphical user interface, text, application

Description automatically generated

Both of the above techniques are extremely useful and relevant when using a Genetic Algorithm (GA) [12] as the main algorithm for this reproduction method.

Genetic Algorithms, as well as some other methods such as NeuroEvolution of Augmenting Topologies (NEAT) [13], will be discussed later in this paper’s literature review (Section 2.3).

2.2 Neural Networks and Deep Learning:

Neural Networks (NN) [14] are the core component to a lot of A.I. applications and take inspiration from the neurons within the human (or other mammalian) brains. This meaning that there are neurons that take input from other neurons and depending on the signal provided, produce some sort of output that is either strong enough to trigger an action or is too weak to do anything, and some other actions is taken.

How is this concept applied to computation?

To digitize this concept of a neuron, the first thing to be done is find a neat way to represent this neuron in a computer system. The representation of this neuron consists of the value of the node, and a set of weights and biases associated with each incoming node used to signify the strength of a certain node (or neuron) similarly to how connections in the human brain can be strong and weak.

Diagram

Description automatically generatedFigure: 3 (Simple Neural Network (Visualisation created using: <http://alexlenail.me/NN-SVG/index.html>))

In Figure 3 above, an extremely basic NN topology is provided to help aid in visualizing how these weights and biases link the inputs to outputs. Just two inputs, x1 and x2 are connected to an output node, x3 and both of these connections have a random weight (when initially assigned) w1 and w3 with the output node x3 also having a bias attached to it, b1. Together, using the input values, weights and bias the value of the output can be calculated. The formula for this is single node as follows:

This is repeated for all nodes in a given layer, Figure 3 only needs this computed once for the single output, but if there were more outputs, or this was a hidden layer with multiple nodes the calculation may need to be computed for 3, 4 or n many times for the size of the new layer.

Training a Neural Network can involve many different techniques, such as some explained in sections 2.1, with the main method being back propagation for a supervised learning technique.

Back propagation is performed after a forward pass of a given network has been completed and the predicted results are compared to the actual results in the training set of data. At the core of this method is the concept of ‘loss’ which is essentially the error rate of the network during its forward pass [15], and this is then used to ‘back propagate’ across the network updating the weights using the root mean squared error as it travels back through (other functions/formulas can also be used to back propagate and calculate new values). This means that the next time the forward pass is performed all of the weights will produce a slightly more accurate prediction since this loss alters them slightly in the correct direction of the learning gradient.

Another method of training a Neural Network is using the Evolutionary Learning methods mentioned in section 2.1, with one common evolutionary algorithm being Genetic Algorithms, which will be explained in section 2.3 of this report.

Most NN’s are much more complicated than Figure 3 shows and tend to look more like Figure 4 (below), with many more layers creating a Deep Neural Network.

Figure: 4 (Complex Neural Network)

Diagram

Description automatically generated

Deep Neural Networks (DNN) and Deep Learning are still in essence extremely similar to usual Neural Networks and learning; however, they operate on a much larger scale. DNNs are architecturally the same as a normal Neural Network however, they have many more hidden layers between the input and output. For example, a normal Neural Network can have 0 or 1 hidden layers, and if there are 2 or more hidden layers, this then constitutes as a Deep Neural Network. Thanks to the extended network of neurons, a Deep Neural Network is much more able to adapt to more complex tasks and learn much more intricate or specific scenarios by tuning all of its parameters. This explains the popularity of Deep Learning as it can be applied to almost any problem and given the correct training data, a DNN could produce extremely accurate results, sometimes much better than humans in some tasks.

With this larger topology of Neural Networks, the usual training method of back propagation does not always work as the loss can diminish as it travels further up the network, thus is not able to alter the weights correctly. These networks can also (if the correct training method is used) be overfit if there is not enough data to train the network, meaning that the size of a network can also be slightly dependent on the data provided to it.

To solve this loss training problem, a solution called a residue block can be implemented to ensure the strength of the signal/loss is not lost. In simple terms, this allows the signal to be passed back along a network separately from the signal/loss that is also being used to process the changes needed to the weights.

Figure 5: (Residue Block)

Diagram

Description automatically generated

Employing this method allows for these larger networks to be trained effectively and make proper use of their size and capabilities with more layers and nodes. An example of a network that operates this way is the ResNet [16] architecture.

2.3 Genetic Algorithms (and NEAT):

2.3.1 Genetic Algorithms

Genetic Algorithms (GA) [17] are a popular form of evolutionary learning that as mentioned in section 2.1 take direct inspiration from Darwinian evolution and apply this technique to how the network is modified and evolves to create a better performing Neural Network. This algorithmic technique takes all of the key concepts from the whole of evolutionary learning and applies them, such as the cross-over and mutation functions.

GAs use chromosomes to represent the attributes within a network take some genetic operators to help guide the population of individuals into the correct direction to reach a global optimum [18]. Parameters are initialized to be a random set, for a Neural Network this would mean initializing a random set of weights and biases to fit the size of the network that is desired, with each of these values being the genes or chromosomes to be used within the GA.

Once the population have been tested and run, each will have gained a fitness value calculated by their performance within the given task, some examples of parameters to factor in while creating the fitness function could be the accuracy of the output or time taken to perform the task at hand. Next the parents of the next generation are selected using these fitness values, with a higher value being the better performing individuals, therefore giving them a higher chance of being picked for the cross-over. Alternatively, the top 2 or 3 performing individuals can be picked, removing the chance element of the selection process, ensuring the best genes are carried into the next generation.

An explanation on selection methods:

As mentioned, there are multiple different ways to select the parents for the next generation of individuals, each providing a different twist on how they are selected, and thus producing different and diverse populations.

Roulette wheel selection [19]:

Roulette wheel uses a chance selection meaning that it is not guaranteed to always pick the best parents for the next generation, however it does keep a more truly random aspect to how the population evolves over time. The better an individual performed the more likely it will be to be picked (it takes a larger portion of the ‘pie’), since these percentages are taken from the fitness of the individual against all others.

Figure 6: Roulette Wheel Selection

Chart, pie chart

Description automatically generated

Elitism [19]:

Elitism, as the name suggests, picks the best individuals and chromosomes and uses these in the new population to ensure that the best genes are always carried through into the next generation. Since the best genes are always carried over, this means that the GA will evolve extremely rapidly allowing for fast convergence on a solution.

Rank Selection [19]:

Ranking takes the fitness of the individuals and sorts then in order of best to worst (best having the highest fitness score, worst the lowest) and then uses these rankings to pick out the induvial to use. For example, the worst may be rank 1, and best rank *N* with *N* being the number of individuals in the population, then the probability that an individual is chosen is proportional to its rank within the population so that no one individual will have an 80% or 90% chance of being picked.

In a pseudo-code format this could look something like:

Figure 7: High level pseudo-code of a Genetic Algorithm

initialize individuals with random weights

while **min** **performance** **NOT** met:

for each **individual** in the **population:**

perform the task

evaluate performance

save fitness value to the individual

end for

select best **individuals** from **population**

for **newIndividual** in **newGeneration:**

select crossover point

swap genes and save as **newIndividual**

**mutate** one chromosome with ***x*** random chance

end for

end while

Figure 6 above uses the single point cross-over technique, but this simple pseudo-code algorithm can be easy adapted to use any cross-over technique, such as uniform cross-over described in section 2.1, or two-point cross-over.

The GA technique can be applied to a multitude of applications, with a good application of this technique being optimization problems [20]. GAs are also preferred for these types of optimization problems over the more well known for optimization problems, such as heuristics since the GA can scale with the problem size in a much nicer way, the scaling is more linear than the alternative heuristic method (this is for larger NP problems) [20].

GAs can also be used in the field of autonomous driving [21] [22] [30], which will be the most relevant for this project.

Section 2.3.2: Exploring NeuroEvolution of Augmenting Topologies:

NeuroEvolution of Augmenting Topologies (NEAT) [23] is an extension of Topology and Weight Evolving Artificial Neural Networks TWEANNs (which is an evolution of sorts from a GA) and operate in a very similar way, however, have one large key difference during the reproduction and mutation phase.

History markers [24] are one of these additions that drastically increase the capabilities but also the complexities of this algorithm. In essence, history markers keep track of the ancestors of different individuals preventing a matching during cross-over that is incompatible, meaning that two individuals may have evolved from a different ancestor and therefore contain different genes (a different topology) resulting in the loss of one of these extra genes during the cross-over phase. These markings ensure that two induvial are mated (crossed over) with each other if they have the same ancestry, preventing the loss of any of these newly evolved genes which could lead to a better overall solution.

Leading on from the historical markers is the addition of speciation to the algorithm. Speciation is useful because when a new gene is added to the network, this can actually have a negative effect of the performance and the fitness of the individual to perform the given task, but with speciation different genes can be placed into a separate category. Individuals then compete within their own species category rather than with the global population, allowing it to develop and improve before being placed against the entirety of the population.

In order to produce these different species, the NEAT algorithm has to able to add/create them at some point. This is performed in the same way to normal weight value mutations, and also performed at the same time as these more basic mutations of the network. Mutations with NEAT can also add whole new genes/chromosomes (weight nodes) or new connections between existing genes. This is how the new species of networks evolve, and why the need for the historical markers and speciation is so integral to NEAT to keep the network improving and exploring as many different avenues as possible.

Diagram

Description automatically generatedFigure 8: NEAT adding a new gene (node)

Diagram, schematic

Description automatically generatedFigure 9: NEAT adding new connection between genes (nodes)

Initialization of the networks in a NEAT algorithm also start as extremely basic [25], and the more complex forms of the network only come as a result of running the algorithm itself and not a preset network topology like would be designed in a normal Neural Network or the more basic Genetic Algorithm.

NEAT can also be extended to deep learning [26], by treating not each node as chromosome but each individual layer as its own chromosome. To translate a DeepNEAT into a normal Deep Neural Network each chromosome in the NEAT algorithm is translated into its respective layer using a set of parameters to do so. A set of hyperparameters are also stored about each chromosome that can then be applied to the entire network, some of these hyperparameters being the learning rate of the network/algorithm.

2.4 Methods for Automated Vehicles:

Automated vehicles have rapidly grown in popularity among businesses and the public over the past decade thanks to some companies like Tesla commercializing this new technology and putting it as an option in their own cars.

There are 5 levels to vehicle automation, each with a different amount of computer input compared to human driver input into the vehicle control [27].

Figure 10: Table of automation levels

|  |  |
| --- | --- |
| Level of Driving Automation | Description of the artificial control |
| 1: Driving assists | Automation provides slight aids, such as lateral assistance (lane assist), or longitudinal assistance to drivers |
| 2: Partial automation | Automation performs **both** lateral and longitudinal assistance to drivers |
| 3: Conditional automation | Automation performs Dynamic Driving Tasks (DDT) |
| 4: High automation | Automation performs DDT and DDT fallback |
| 5: Full automation | Automation performed full DDT with DDT fallback as well as Operational Design Domain (ODD) |

From [27] SAE 2016 states that DDT is these subtasks: 1) Lateral vehicle motion, 2) longitudinal vehicle motion. 3) monitor the driving environment using object detection and event detection, recognition, classification and response preparation, 4) object and event response execution, 5) maneuver planning.

Autonomous vehicles need to be able to ‘see’ the environment they are in, so that they can make informed decisions about where to go, where is free of other traffic, where other cars are on the road, if there is an obstruction or pedestrian in the way. To do this, some different vision techniques can be applied to a car either combined, or individually, with the two main systems for a cars vision being LIDAR and Cameras [28]. Both of these methods have their strengths, for example, the cameras on an autonomous car can be used to detect objects within the environments, which for use on public roads is extremely important so that a car can see road signs or traffic lights and act accordingly, as well as react to other cars or pedestrians moving around. LIDAR sensors are useful for calculating 3D point distances within the environment, therefore are able to give the car the special awareness it will need to navigate safely around any obstacles, as well as plan paths correctly, by knowing how far a certain object (even if it does not know what it is just by lidar data) is and how fast it is going. Using this data, localization [29] can also be performed.

These methods are used in conjunction for self-driving cars to be used on public roads due to the complexity of the challenge of driving on a road with other road users and a potentially unlimited number of uncertainties that come with this activity. The cameras object detection capabilities can be used not only to detect certain objects like pedestrians, as mentioned, but also to detect the roadway to drive on. This can then be used in path planning for the vehicle, that can then choose one of these paths to follow that could be either; least obstructed, fastest lane for a corner or just keeping the vehicle in a safe spot on the road, while also following the route to the destination.

Methods for creating autonomous vehicles:

Deep learning is often used in autonomous vehicles [30] due to their complexity, and the extra complexity of a deep network and deep learning caters for this well. The task of controlling a vehicle can be broken down into two main tasks which are lateral vehicle control (i.e. steering, turning the vehicle) and longitudinal vehicle control (i.e. accelerating and braking the vehicle). Deep learning is paired with the images captured by the car, which are then passed into a Neural Network, most likely in this case for image and object detecting a Convolutional Neural Network (CNN).

Figure 11: Simple CNN

Diagram

Description automatically generated

This method of learning for a self-driving car usually utilizes the supervised learning method, given that you can have labelled images of pedestrians, the road and other cars fed to the CNN which can then learn to recognize all of these different objects. Using this method even calculations of steering angles can be calculated from the detection of road and pathways. This means that, even though the A.I. and Neural Network is mostly trained on just recognizing images, it can be expanded to allow for accurate vehicle controls to be determined through what it finds within an image, whether that be braking for a traffic light, or turning to avoid a collision, to accelerating onto a motorway.

CNNs are the one of most popular deep learning method for autonomous with already known CNNs, such as GoogLeNet [31], being used to recognize all objects within an image for the car.

However, supervised deep learning requires immense amounts of data to accurately train the networks involved to give reliable and acceptable outputs [30], which can be difficult to come by for the autonomous driving area.

Evolutionary learning (NeuroEvolution) is also one method that can be applied to an autonomous vehicle [32]. To create an autonomous vehicle using this method however, real life applications cannot be used during any sort of training phase, as this sort of technique starts of not ‘knowing’ anything, therefore would not be safe to use on real roads, or tracks. Due to this, a simulation is used to first train the A.I..

GAs used for autonomous driving can be used in both an ‘empty’ [32] road simulation and a ‘busy’ road [33] simulation, proving that this technique can be used for a range of complexities within the self-driving area, and with some further development, these simulations could be expanded to control real vehicles on public roads safely. This method can however lack some of the preciseness needed for a truly safe real road autonomous car, meaning that it is the best method for creating a baseline to fine tune and increase the robustness from, as an autonomous car created from a GA learns the basics of collision avoidance and car maneuverability much faster than any other method.

NeuroEvolution and GAs also benefit from not needed hundreds of thousands of data to learn from, as they learn and evolve from their own experiences by choosing the two best performing individuals, meaning for an autonomous driving task, a GA can be extremely helpful if there is limited data to develop and learn from. The GA can learn the basics of the task through its own evolution and then this agent can be further tweaked by any extra data and techniques to ensure a robust and safe operating vehicle is created.

Section 3: Methodology used

In my own autonomous car simulation, I will be using these two key technical A.I. based components: Deep Neural Networks (DNN), and a Genetic Algorithm to evolve and train the cars.

Due to the complexities of the task that I am training the car to overcome (despite it being a relatively simple autonomous car, the task is still complex) a Deep Neural Network most likely will be required. A DNN will be able to tune more parameters within the network itself, meaning that the car can adapt to more stimuli as well as make more fine-tuned adjustments, for example, whilst turning a corner, the DNN would be able to better adapt to a change in angle, or speed if it were moving too fast. The nature of the track it will be learning means that this adaptability is crucial as Cadwell Park contains a large variety of corners, angles of said corners and straights.

Figure 12: Cadwell Park Outline

Diagram

Description automatically generated

Using this in combination with a Genetic Algorithm will also mean that the solution for training the DNN will be much simpler and will not require the implementation of a residue block to store any ‘loss’ value. No ‘loss’ value will be generated as there will be no back-propagation through the network. However, the complexities arise when trying to find an adequate fitness function to evaluate the performance of each car as it attempts to navigate and drive around the track.

The reason I will be implementing these two techniques for the autonomous car is because as stated, autonomous vehicles are a complex form of Artificial Intelligence, so will benefit greatly from the extra flexibility that the DNN will offer, over a basic Neural Network with no hidden or only one hidden layer.

As part of the project, I will be exploring how different complexities and sizes of networks affect the car, whilst also trying to find the best possible topology for the network to be to control the car in the best way possible, as will be judged by the fitness function.

I also want to explore the area of Evolutionary Learning and implementing a Genetic Algorithm will be the perfect way to discover this new area of Machine Learning and A.I. to me, and a relatively new development in Artificial Intelligence as a whole. On top of this, while there were some autonomous vehicle papers that used Evolutionary Learning and Genetic Algorithms to develop their own car simulation, and some other examples I managed to find online using Genetic Algorithms or NEAT to create an autonomous vehicle, in comparison to some other methods Evolutionary Learning has been used less. This could be because of the novelty of Evolutionary Learning, and/or that supervised learning, using cameras to detect object within a vehicles field of view has already been established as a robust method for creating reliable autonomous vehicles.

Despite this, I still want to explore the potential of Evolutionary Learning with autonomous vehicles in hopes to better understand Evolutionary Learning as a whole and how to adapt this technique to be used in a lesser explored field and build upon the knowledge already found for using this technique for this application.

One more reason for this evolutionary approach, is because there is no data that I can use to train a network off that would match the environment the car will be driving in. Meaning that, it will not be possible to explore a supervised learning method, unless I drove the car around the track in Unity hundreds, if not thousands of times myself, but this is not practical to do to collect data. Therefore, the lack of training data, means that Evolutionary fits well here as it learns from its own experience, rather than others own experiences.

The more basic Genetic Algorithm will be enough for this task when compared to the NEAT evolutionary algorithm, since the network, despite being a DNN, will not need to be immensely complex for this task. Within this GA, I will be using uniform cross-over to create the next generation of cars from the parents, which will start out as just the two best (using elitism) of the current generation to be these parents.

For the fitness function this algorithm will use to calculate each cars performance will first start out as:

Or more commonly known as the average speed. This will be the first fitness function I try (but subject to change depending on its effectiveness on producing successful cars) because I want to try and create a car that not only can navigate around the course successfully, but also do so in a fast manner, trying to as closely as possible, replicate a real drive around the track.

To implement these techniques, I will be using a combination of software and programming languages.

I will be using Unity3D to host the simulation of the track and vehicle.

Unity is a free game development software that allows for easy creation of game like applications, which will be similar to what I will be making with my simulation. It also, due to its popularity, has lots of support online through its own documentation and community support, in terms of posts on forums, and online video tutorials. As I’m not 100% familiar with the language used (C#) this will be very helpful to me, however, I do want to expand my knowledge base of programming languages so using C# is also a bonus for me to learn a new programming paradigm.

For the A.I. and GA I will be implementing, I have chosen to create this out of the Unity code space and implement it with Python. The reasoning for this is because I am already very familiar with this language thanks to multiple modules that have used this language throughout university and with many modules using Python for Artificial Intelligence applications, allowing me to transfer knowledge I have gained from other modules into this final project to show my development and learning over the past years.

Section 4: Implementation

On a more detailed level, within the Unity project I will import the 3D model of Cadwell Park from Blender that I will create myself as well as all of the distance gates that will be used to measure how far the car has travelled. Then once imported, I can label them all as ‘Track’ for the track and ‘marker’ for the distance markers/gates. Using these tags within Unity, I can calculate when a collision occurs with the track walls, and when the car passes through a distance gate. Upon a collision with the track walls, the car will be reset to its original position, and all physics acting upon it reset, so that the next car is able to start off in the same way as all of the other cars, creating a fair environment for each vehicle to compete in. To reset the physics in Unity I set the attribute ‘*isKinematic*’ to **true**, then **false** after the car had been reset. This attribute is a value a Rigidbody object contains that allow or disallow physics operations to be performed on this object, when true, no physics affect the object, when false, physics are calculated for the object, hence why turning this on then off during a reset resets all physics currently acting on the car.

All a Rigidbody means in unity is that if an object belongs to this class, the Unity physics engine acts upon it.

Figure 13: Cadwell in Unity (View from above)

A drawing on a blackboard

Description automatically generated with low confidence

As shown, this is a very close recreation of the real track, minus the verticality of the track (this is a flat replica, without any hills).

For the car itself, I found a free 3D model of a Toyota GT86 on the Unity asset store that I then downloaded and imported into the project. This car used WheelColliders mounted onto the wheel objects to control its movement. With these components, you can create a more accurate representation of how a car will act, although they do require more knowledge to control, rather than some other ways of moving a Rigidbody object.

With these wheel colliders however, I can control many aspects of the car such as the suspension stiffness, and travel, grip/friction each wheel has before traction is broken, both longitudinally and laterally, (forwards/backwards and sideways (left/right)) and even the mass of the wheel itself. Within the code and setup of these objects, I can also set the values for the ‘engine’ power of the ‘brake’ power, that when applied to these colliders propel the car in a more realistic manner. Most values of the WheelColliders themselves are default, with a slight increase in the slip values for friction (in the forwards direction) giving more traction to propel the car, and an increase in lateral stiffness of the car for turning.

Given that the cars weight is set at 1000Kg (1 tonne), I have given the following constants the values of:

* MAX\_STEEL\_ANGLE = 45 (45-degree maximum turn angle for the front wheels)
* ENGINE\_POWER = 1500 (maximum power available to the rear wheels (since this car is rear wheel drive))
* FRONT\_BRAKE\_POWER = 1000 (maximum brake power of the front wheels brakes)
* REAR\_BRAKE\_POWER = 750 (maximum brake force of the rear wheel brakes)

These values are all set via in the scripts (programmatically, in C#) rather than in the unity editor itself.

The front wheels have a greater braking force to mimic how modern cars are created, with a larger set of brakes for the front wheels, since this is where most of the braking is done, due to the weight transfer to the front wheels during the braking process. The control of the direct components on the car is performed in the ‘*CarController.cs*’ file of the project.

To control all of these components, I create a ‘*WorldState*’ (‘*WorldState.cs*’) to keep knowledge of the environment and the car, such as the speed of the car, distance travelled, as well as the starting position and rotation of the car for when it needs to be reset.

Attached to the cars Rigidbody are a set of 9 cubes (that are invisible) that each shoot out a ray in a given direction related to the direction the car is facing. These are the rays used to imitate LIDAR that is often used in real autonomous vehicle situations and will be measuring the distance from each of these cubes (ray origin points) to the nearest first collision point with the track.

Figure 14: Rays shot from car

A picture containing sky

Description automatically generated

In conjunction with the speed of the car, this will total the 10 inputs into the DNN.

In order to connect the Unity simulation to the Python A.I., I first thought of using HTTP requests, since this is an easy way to send and receive data between two applications. Both Unity and Python have modules that can assist with this technique as well, ensure a simple implementation into the project. However, this method can sometimes be slow, which for a real time application and simulation such as this could cause performance issues.

In the end I decided to proceed with a WebSocket. A WebSocket will be able to transfer between the two applications faster than traditional HTTP since a connection, once started, is always open between the two applications, and there is no ‘sender and receiver’ like in the HTTP method. Both software and languages I am using have support for WebSockets too, natively, without installing any third-party packages, which, whilst making the implementation a little more complex due to the nature of the sockets, still completely possible with a lot of documentation for both Unity and Python in this area.

To use the WebSocket, I also had to implement a method to determine the end of a data stream sequence, since not all of the data was always sent in one packet. Therefore, I had to use delimiters at the end of each data object that was sent to and from Unity and Python. The data sent was in a JSON object format, which also helped make it easy to determine the start and end of the actual data sent, I used this notation with a delimiter of ‘**|**’ to indicate the end of the object, and when this was encountered, processing of the data on either end could begin, and any extra data was ignored. Using this allowed me to ensure that the correct amount of data would be used without any missing, or extra items.

Constructing the Neural Network and Genetic Algorithm were all performed in Python thanks to the large support online as well as some extremely helpful packages that can be installed and imported to help with the processing, calculations and creating of such networks. I mainly and only used the package NumPy to aid with the Neural Network aspect of this project, since, if I used more packages to create and control the evolution of the Neural Networks, such as PyTorch, then I would not have had the total control that I had creating it all myself.

To create these networks, I specified the seize of each layer, and created a NumPy array to this specification to match each of the weights, and biases that would be needed for each layer-to-layer connection. For example, a layer of size 5 connected to a layer of size 3, would require 15 weights to connect them all up, into a fully connected layer. I then save all of these networks to JSON files to easily visualize the network layout, and so I can easily keep the fitness of each car within the cars own network file.

While performing the forward pass of the network, I first need to normalize the data given from Unity passed via the WebSocket. While testing the car controller, I was able to find theoretical maximum distances each of the rays could detect, as well as the maximum speed of the car, so I used these to normalize the data to between 0 and 1 so that there would not be any value that overpowers the system. I used Min-Max normalization to normalize the data, for example: .

Once the data has been normalized and is within the appropriate scale, it is sent through the network. To calculate the outputs of each of the nodes, and layers I used the NumPy function ‘*np.sum*’ on the combined array of weights and inputs into the layer (for layer one, this is the inputs from the car) by using the ‘*np.array*’ function. Using NumPy to help with the calculations is ensures that during run time, the calculations are performed extremely quickly, allowing the simulation to run in real time. Evidence of this is the frame rate of the simulation in Unity, that was able to reach over 150, and close to 200 Frames Per Second at points.

The outputs of each node were also passed through a modified sigmoid function.

This modified sigmoid allows valued between -1 and 1, where any value below 0 is braking, or turn left, and above is accelerate or turn right.

The **final output** of the network is **two nodes**, each with a value being between **-1 and 1**. The first node supplies the value to the accelerator/brake, and the second node is the turn value. This is then sent back to Unity via the WebSocket where they are then fed to the car controller. For example, the acceleration would be the (brake power is triggered if the output is less than 0), so if the output is 0.5 from the network, this will equate to half throttle and -0.5, is half brake power. The same is for the turn angle, this is multiplied by the output value from the network, so a value of -0.25 from the network is -0.25\*45 (the maximum turn angle).

Figure 15: Output of the Neural Network

Diagram

Description automatically generated

This would indicate a left turn of moderate angle, and a slight acceleration.

After a car crashes, the fitness is determined using the fitness function which is the saved to the same car file the network is saved in.

Upon completing a generation, the Genetic Algorithm is run. To perform uniform cross-over, the two parents, already determined by their fitness are taken and on a random chance, 50/50 (so equal between the two)

Section 5: Results

Section 6: Conclusion and Further Work

References

[1] Schrider, Daniel R., and Andrew D. Kern. "Supervised machine learning for population genetics: a new paradigm." *Trends in Genetics* 34.4 (2018): 301-312.

[2] LeCun, Yann, et al. "A theoretical framework for back-propagation." *Proceedings of the 1988 connectionist models summer school*. Vol. 1. 1988.

[3] P. Sharma, D. Austin and H. Liu, "Attacks on Machine Learning: Adversarial Examples in Connected and Autonomous Vehicles," 2019 IEEE International Symposium on Technologies for Homeland Security (HST), 2019, pp. 1-7, doi: 10.1109/HST47167.2019.9032989.

[4] Fridman, Lex. "Human-centered autonomous vehicle systems: Principles of effective shared autonomy." *arXiv preprint arXiv:1810.01835* (2018).

[5] O'Shea, Keiron, and Ryan Nash. "An introduction to convolutional neural networks." *arXiv preprint arXiv:1511.08458* (2015).

[6] Chiaroni, Florent, et al. "Self-supervised learning for autonomous vehicles perception: A conciliation between analytical and learning methods." *IEEE Signal Processing Magazine* 38.1 (2020): 31-41.

[7] M. Usama et al., "Unsupervised Machine Learning for Networking: Techniques, Applications and Research Challenges," in IEEE Access, vol. 7, pp. 65579-65615, 2019, doi: 10.1109/ACCESS.2019.2916648.

[8] N. Grira, M. Crucianu, and N. Boujemaa, ‘‘Unsupervised and semisupervised clustering: A brief survey,’’ Rev. Mach. Learn. Techn. Process. Multimedia Content, vol. 1, pp. 9–16, Jul. 2004.

[9] Aristidis Likas, Nikos Vlassis, Jakob J. Verbeek, The global k-means clustering algorithm, Pattern Recognition, Volume 36, Issue 2, 2003

[10] J. Zhang et al., "Evolutionary Computation Meets Machine Learning: A Survey," in IEEE Computational Intelligence Magazine, vol. 6, no. 4, pp. 68-75, Nov. 2011, doi: 10.1109/MCI.2011.942584.

[11] Sacha Gobeyn, Ans M. Mouton, Anna F. Cord, Andrea Kaim, Martin Volk, Peter L.M. Goethals, Evolutionary algorithms for species distribution modelling: A review in the context of machine learning, Ecological Modelling, Volume 392, 2019

[12] F. H. F. Leung, H. K. Lam, S. H. Ling and P. K. S. Tam, "Tuning of the structure and parameters of a neural network using an improved genetic algorithm," in IEEE Transactions on Neural Networks, vol. 14, no. 1, pp. 79-88, Jan. 2003, doi: 10.1109/TNN.2002.804317.

[13] L. Chen and D. Alahakoon, "NeuroEvolution of Augmenting Topologies with Learning for Data Classification," 2006 International Conference on Information and Automation, 2006, pp. 367-371, doi: 10.1109/ICINFA.2006.374100.

[14] Bishop, Chris M. "Neural networks and their applications." *Review of scientific instruments* 65.6 (1994): 1803-1832.

[15] Vogl, T.P., Mangis, J.K., Rigler, A.K. *et al.* Accelerating the convergence of the back-propagation method. *Biol. Cybern.* **59,**257–263 (1988). <https://doi.org/10.1007/BF00332914>

[16] Targ, Sasha, Diogo Almeida, and Kevin Lyman. "Resnet in resnet: Generalizing residual architectures." *arXiv preprint arXiv:1603.08029* (2016).

[17] Holland, John H. “Genetic Algorithms.” *Scientific American*, vol. 267, no. 1, 1992, pp. 66–73, [http://www.jstor.org/stable/24939139. Accessed 6 Apr. 2022](http://www.jstor.org/stable/24939139.%20Accessed%206%20Apr.%202022).

[18] Adaptive and Natural Computing Algorithms, 8th International Conference, ICANNGA 2007, Warsaw, Polamd, April 11-14, 2007, Proceesings, Part II, Bartlomiej Beliczynski, Andrzej Dzielinski, Marcin Iwanowski**,** Bernardete Ribeiro

[19] Haldurai, L., T. Madhubala, and R. Rajalakshmi. "A study on genetic algorithm and its applications." *International journal of computer sciences and Engineering* 4.10 (2016): 139.

[20] Bhoskar, Ms Trupti, et al. "Genetic algorithm and its applications to mechanical engineering: A review." *Materials Today: Proceedings* 2.4-5 (2015): 2624-2630.

[21] Arrigoni, Stefano, Francesco Braghin, and Federico Cheli. "MPC path-planner for autonomous driving solved by genetic algorithm technique." *arXiv preprint arXiv:2102.01211* (2021).

[22] Jalali, Seyed Mohammad Jafar, et al. "Optimal autonomous driving through deep imitation learning and neuroevolution." *2019 IEEE International Conference on Systems, Man and Cybernetics (SMC)*. IEEE, 2019.

[23] P. Caamano, F. Bellas and R. J. Duro, "Augmenting the NEAT algorithm to improve its temporal processing capabilities," 2014 International Joint Conference on Neural Networks (IJCNN), 2014, pp. 1467-1473, doi: 10.1109/IJCNN.2014.6889488.

[24] Chen, Lin, and Damminda Alahakoon. "NeuroEvolution of augmenting topologies with learning for data classification." *2006 International Conference on Information and Automation*. IEEE, 2006.

[25] Ibrahim, Mohamed Yilmaz, et al. "Advances in neuroevolution through augmenting topologies–a case study." *2019 11th International Conference on Advanced Computing (ICoAC)*. IEEE, 2019.

[26] Risto Miikkulainen, Jason Liang, Elliot Meyerson, Aditya Rawal, Daniel Fink, Olivier Francon, Bala Raju, Hormoz Shahrzad, Arshak Navruzyan, Nigel Duffy, Babak Hodjat, Chapter 15 - Evolving Deep Neural Networks, Artificial Intelligence in the Age of Neural Networks and Brain Computing

[27] Inagaki, Toshiyuki, and Thomas B. Sheridan. "A critique of the SAE conditional driving automation definition, and analyses of options for improvement." *Cognition, technology & work* 21.4 (2019): 569-578.

[28] S. Kato, E. Takeuchi, Y. Ishiguro, Y. Ninomiya, K. Takeda and T. Hamada, "An Open Approach to Autonomous Vehicles," in IEEE Micro, vol. 35, no. 6, pp. 60-68, Nov.-Dec. 2015, doi: 10.1109/MM.2015.133.

[29] M. Betke and L. Gurvits, "Mobile robot localization using landmarks," in IEEE Transactions on Robotics and Automation, vol. 13, no. 2, pp. 251-263, April 1997, doi: 10.1109/70.563647.

[30] S. Kuutti, R. Bowden, Y. Jin, P. Barber and S. Fallah, "A Survey of Deep Learning Applications to Autonomous Vehicle Control," in IEEE Transactions on Intelligent Transportation Systems, vol. 22, no. 2, pp. 712-733, Feb. 2021, doi: 10.1109/TITS.2019.2962338.

[31] M. Al-Qizwini, I. Barjasteh, H. Al-Qassab and H. Radha, "Deep learning algorithm for autonomous driving using GoogLeNet," 2017 IEEE Intelligent Vehicles Symposium (IV), 2017, pp. 89-96, doi: 10.1109/IVS.2017.7995703.

[32] Sainath, G., et al. "Application of Neuroevolution in Autonomous Cars." *International Virtual Conference on Industry 4.0*. Springer, Singapore, 2021.

[33] Trasnea, Bogdan, et al. "GridSim: A vehicle kinematics engine for deep neuroevolutionary control in autonomous driving." *2019 Third IEEE International Conference on Robotic Computing (IRC)*. IEEE, 2019.

[34] Li, Yuxi. "Deep reinforcement learning: An overview." *arXiv preprint arXiv:1701.07274* (2017).

[35] Sutton, Richard S., and Andrew G. Barto. "Reinforcement learning." *Journal of Cognitive Neuroscience* 11.1 (1999): 126-134.

[36] Watkins, Christopher JCH, and Peter Dayan. "Q-learning." *Machine learning* 8.3 (1992): 279-292.